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Site Access and Safety Protocol
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Pre-visit requirements, PPE matrix, and permit controls.

Pre-Visit Requirements
Confirm site contact, access window, RAMS status, and required permits before attendance.

PPE Matrix
Minimum PPE includes safety footwear, eye protection, and task-specific equipment as required
by site risk profile.

Permit Controls
No high-risk works commence until permit-to-work is approved and logged by authorised
personnel.

Isolation Procedure
Follow lock-off and test-for-dead sequence before intervention on energised systems.

Sign-off
Complete safety sign-off, update records, and report any residual hazards before leaving site.

Contact
T: 01202 028 869
E: info@apluselectrical.co.uk
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